# **Defects Of Coffee Vending Machine.**

* Verify that the dimension of the coffee machine is as per the specification.
* Verify that outer body, as well as inner part’s material, is as per the specification.
* Verify that the machine’s body colour as well brand is correctly visible and as per specification.
* Verify the input mechanism for coffee ingredients-milk, water, coffee beans/powder, etc.
* Verify that the quantity of hot water, milk, coffee powder per serving is correct.
* Verify the power/voltage requirements of the machine.
* Verify that coffee should not leak when not in operation.
* Verify the amount of coffee served in single-serving is as per specification.
* Verify that the digital display displays correct information.
* Check if the machine can be switched on and off using the power buttons.
* Check for the indicator lights when the machine is switched on-off.
* Verify that machine should not make too much sound when in operation.
* Check the amount of time the machine takes to serve a single serving of coffee.
* Check the performance of the machine when used continuously until the ingredients run out of the requirements.
* Check the functioning of the coffee machine when two/multiple buttons are pressed simultaneously.
* Check the functioning of the coffee machine if the ingredient container’s capacity is exceeded.