# **Defects of Door!!**

### Wood Attacking Pests.

* Wood with Dead Knot.
* Cracks in Door Panel/Frame.
* Peeling off Laminate.
* Peeling off Paint or paint deterioration.
* **Improper Alignment of Frames.**
* **Stability.**
* **Excessive Gap under Door Panel.**
* **Inadequate Fasteners at The Frame.**
* **Gap around Door Frame.**
* **Loose Fittings.**
* **Open/Close.**
* **Lamination.**
* **Floor Level.**
* **The lock.**
* **Weak handle.**
* **If the door is double side open and close then the door has to work properly both of the sides.**
* **If the door is made of glass, then the door has to be strong.**
* **Check the edges of glass door it should be soft not sharp.**
* **If the door is sliding door, then the slider would have to work properly.**